********************
Function and Control
********************

This function is only supported for C9100-12/13/14 cameras. For C9100-12, the newer firmware may be required to use this mode in the camera. If you are using C9100-12, please check with Hamamatsu if you require this mode.

1. Import Phoenix internal.emulation+.reg to force the camera to run internal trigger mode using software trigger. The result of this effect will allow the camera to be able to expose down to about 1ms exposure in internal mode. A side effect of this mode is that the camera can no longer run in overlap exposure mode. This is due to the fact that this camera uses a frame transfer CCD and has no electrical shutter so only non-overlap is possible to achieve exposures less than 1 frame readout time. The result is exposures which are close to readout time or larger will output at a slower frame rate than overlap true internal mode.
2. Import Phoenix internal.emulation-.reg to force the camera to run internal trigger mode back to the default overlap exposure mode with maximum frame rate.

