********************
Function and Control
********************

1. Import 1394OHCI internal.emulation+.reg to force all 1394 cameras to run internal trigger mode using software trigger. The result of this will help prevent image skewing during internal trigger capture when ccErr_lostframe errors / packet loss occurs. A side effect of this mode is that the camera data rate will be slower than the maximum rate the hardware can perform in true internal trigger mode.
2. Import 1394OHCI internal.emulation-.reg to force the camera to run internal trigger mode back to the default with maximum frame rate.