********************
Function and Control
********************

This function is used to change the default External Trigger Source connector on cameras which support Multi 6 or BNC such as ImagEM (C9100-13/14)

1. Import triggersource.bnc.phoenix.reg to force the BNC connector as the default source.
2. Import triggersource.multi6.phoenix.reg to force the Multi 6 connector as the default source.